GMT Aug 20 00:06 V. Bhat - DSL120 backscatter swath, submersible-based observations, and interpretation for Main Endeavour Field [including previous mapping by V. Robigou]

5400

5600

5800

6000

6200

6400

Northing (m)

4600 4800 5000 5200 5400

Easting (m)

LEGEND Live Sulfide Dead Sulfide/Talus/Oxed Sed Diffuse Flow Collapse Features Ropy/lobate/sheet flows Pillows/Generic Basalt Fault/Fissure/Talus Unknown Water Column Instabilities

5400

5600

5800

6000

6200

6400

Northing (m)

LEGEND Active sulfides - semicircular reflectors, ~ 10-20 m wide, 15-20 m high, casting long shadows Inactive sulfides - semicircular reflectors, ~ 10-20 m wide, 2-15 m high, with short, blocky shadows Lineated block - short wavelength/high amplitude backscatter and bathymetry variations Lava lake - very smooth backscatter and flat [often depressed] bathymetry Fissure - Bright/dark backscatter lineation couple, bathymetric trough Top of fault scarp/talus slope [barbs downdip] Base of talus slope Nadir/Edges of sonar swath

5400

5600

5800

6000

6200

6400

Northing (m)

4600 4800 5000 5200 5400

Easting (m)